ID: 20
Name: Documentation_Updates_742
Version: 3.20
Dependences: none
Description: Version 1.0@@@Updated naUsbDevQueue regarding zero-length packets.@@@Version 1.1@@@Added IPv4 filtering@@@Version 1.2@@@Updated USB Host error codes.@@@Updated getaddrinfo and ethernet multicast in bypass mode.@@@Version 1.3@@@Corrected description of serial and SPI signals.@@@Version 1.4@@@Added new API naIpsecIkeSendSaLifetimes which lets users determine if SA lifetime information should be included in the initial IKE message.@@@Version 1.5@@@Enhanced documentation of exception codes.@@@Version 1.6@@@Updated information on IPv4 automatic collision detection.@@@Version 1.7@@@Added an API that allows users to install callback functions which are invoked by the kernel whenever it enters an idle state, or switches to a new thread.@@@Version 1.8@@@Added White Papers@@@Application Note- Ajax programming using Digis Advanced Web Server @@@Application Note- Combining CLib and Native File System APIs @@@Application Note- Controlling Page Changes in AWS @@@Application Note- Creating SSL Certificates @@@Application Note- Javascript Forms Processing with AWS @@@Application Note- Using the Advanced Web Server @@@Application Note- Adding custom MIBs to NET+OS 7.x projects @@@Application Note- Real-time Device Monitoring Using AWS @@@Application Note- Accessing NET+OSs SNMP agent using MGSofts SNMP management Software @@@Application Note- Enabling SNMPv3 Security Features in NET+OS V7.X @@@Application Note- Generating HTML content on the fly with AWS @@@Application Note- Adding DHCP options to NET+OS 7.x@@@Version 1.9@@@Updated API Reference for new link layer status callback flag for serial link down (PPP_LL_LINK_DOWN) @@@Version 2.0@@@Updated API Reference to clarify the usage of the NOR Flash functions.  These functions were shown available for all platforms but are not available on NAND-based platforms (CC9P 9360).  This is now clarified, plus some clean up indicating the topic is Flash and subtopic is either NOR or serial.@@@Version 2.1@@@Added LINKUP and LINKDOWN events. Updated mwifimac for LINKUP and LINKDOWN event and added naWlnSetEvent for wpa to setup linkup and linkdown events and startMultiScan for multiple channel mask scan.@@@Added naEkahauSetBatteryCallback prototype and naEkahauSetStatusCallback API.@@@Added naWlnIsWirelessUp function to see whether wireless is ready to transmit.@@@wlnNullFramePtrPS and wln_make_null_frame_ps are added for background scans while staying associated.@@@Version 2.2@@@Now use the WAKE UP button for forced recovery for the cc9p9215, ccwi9p9215 and the ns9210 modules on the cc9p9215 carrier board. (case 33388)@@@Version 2.3@@@Added description of channel index as it relates to the wireless channel numbers. (case 33515)@@@Added white paper- Application Note- Correcting Linker errors in DIGI ESP@@@Version 2.4@@@Added link to naSetNotificationUserName  (case 33298)@@@Added white paper - Taking Advantage of Digis Advanced Web Servers Repeat Group Feature@@@Version 2.5@@@Added reference to NAgetGPIOpinConfig. (case 34240)@@@Clarified wln_scan_bss structure -> channel description. (case 33226)@@@Version 2.6@@@Added NA_ETH_SET_PACKET_TRAILER_SIZE.  This constant can be used to enable a packet trailer in Ethernet packets. It is normally set to 0 and a trailer is not used.@@@Updated the NS9215 SPI Master driver to implement additional SPI ports using the FIM processors.  This was done to provide a work-around to problems in the internal NS9215 SPI port.@@@Added new roaming API to the Wi-Fi driver.  See API Reference for details.@@@Added Support for WPA2 Mixed Mode. (cases 33127 and 34393).@@@Version 2.7@@@Enhanced documentation related to the FIM CAN Driver.  Added new APIs.  (Case 26317, 32022, 34921)@@@Added white paper- Application Note- Developing CGI-based AWS Applications Using Digis NET+OS Development Environment@@@Version 2.8@@@Added white paper- Application Note- How Changes in MS Internet Explorer Version 8 Will Affect Web Pages Containing Input type=file@@@Version 2.9@@@Added documentation for snmpTargetMIB and snmpNotificationMIB. (Case 36130)@@@Changed description of NASpiSlaveBufferType in ApiReference to state that the SPI receive buffer should be 32-byte aligned. (Case 36111)@@@Updated ConnectME ConnectWiME ConnectME9210 HW Reference to Rev J.@@@Version 3.0@@@Updated FIM SPI clock rates@@@Added new FIM SPI APIs@@@Updated NaSnmpTrap_t  structure.@@@Updated NS9210/NS9215 Errata@@@Version 3.1@@@Added sendBreak process. Updated serl_monitor to send interrupt command to FIM to set TX low for sendBreak and restore TX after given duration has expired. The FIM code was also updated for sendBreak command. Updated actual bytes written TX instead the number of bytes sent to FIM which includes stop bits and parity. (Case 31247)@@@Updated autodoc comments for naIpsecPolicyContentSetRules to explain problem with using IPSEC transport mode and do not fragment option.  Recommended use of IPSEC tunnel mode instead. Also described a work around.@@@Version 3.11@@@Updated NS9210/NS9215 Errata@@@Added NS9210/NS9215 FIM SPI Port Implementation Reference@@@Version 3.12@@@Corrected FIM SPI MISO and CS signals in API Reference@@@Version 3.13@@@Added APIs to allow users to limit the amount of heap the TCP/IP stack is allowed to allocate.  Set the default limit to be half the heap. (Case 40091)@@@Improved documentation for naIsrSetFiq to describe the limitations of FIQ service routines, and to describe the other configuration settings that need to be changed to support an FIQ service routine.@@@Version 3.14@@@Fixed incorrect autodoc description of fLanguagePtr in CGI structure.  (Case 41908)@@@Version 3.15@@@Application Note - Switching between DHCP and Static IP address Acquisition in NET+OS@@@Application Note - Handling multiple submit buttons in NET+OS development environment web-based applications@@@Application Note - JavaScript and pbuilder compression@@@Version 3.16@@@Updated the NS9210, NS9215, ConnectSP and Wi-SP, ConnectME Wi-ME ME9210,  and Connectcore 9P and Wi-9P 9215 Hardware Reference Manuals@@@Version 3.17@@@Application Note - AWS, CSS and id selectors@@@Application Note - Catching Crashes in NET+OS using ESP@@@Version 3.18@@@Updated the Connectcore 9P and Wi-9P 9215 Hardware Reference Manual@@@Version 3.19@@@Removed erroneous note from FCConnect.@@@Version 3.20@@@Removed Constants for SSL Version which became obsolete upon mitigation of the POODLE SSL attack. (NETOS-105)
platformversion: 7.4
Revision: 2
platform: netos
Relevance: NORMAL
Filename: Documentation_Updates_742_20.dipk
Date: 18/11/2014
Type: documentation
Target: environment
neededfiles: none
rootfs: none
minidescription: Documentation Updates for NET+OS 7.4.2
Size: 26812kb
Installedsize: 30646kb
Checksum: 480bfaa5fde9fd3136290a5946dcd89e
