ID: 130
Name: SNMP_Updates_752
Version: 1.11
Dependences: 136
Description: Version 1.0@@@Fix from Treck for getting an OID with bad interface index for IfStatsTable. (Case 39737)@@@Version 1.01@@@Added application API example to access scalar MIB data. (Case 40867)@@@Version 1.02@@@Removed varbind for sysuptime for V1 trap in tfSendNotificationsForEntry. (Case 42182)@@@Version 1.03@@@Fix for SNMP replying to a different IP address, than in received request (IPv6 only)  (Case 43127)@@@Version 1.04@@@Fixed use of broadcast source address in the reply, introduced with fix to case 43127. (Case 44459)@@@Version 1.04@@@Fixed use of broadcast source address in the reply, introduced with fix to Vantive 43127. (Case  44459) @@@Version 1.05               @@@Report correct Ethernet link speed in SNMP ifSpeed  (Case 41612)  Requires TCPIP fix v1.03.@@@Version 1.06@@@Fixed API functions that access SNMPv3 (tablesnaSnmpDeleteS2GEntry and others)  (Case  44459)@@@Disable SNMP printable character testing using  new NET+OS API@@@Version 1.07@@@Replaces direct malloc() and free calls() with tm_snmp_malloc and tm_snmp_free in NET+OS snmpv3 api. (NETOS-39)@@@Version 1.08@@@Fixed a bug in how the SNMP agent handles certain SNMPv3 requests.  According to RFC-3414, when we receive a request with the authentication bit set, the  privacy bit clear, the engine boots set to 0, and engine time set to 0, the  agent is suppose to respond with a wrong timeliness report.  That request/report combination is used by the manager to get the current engine boots and engine time values from the agent.  We were sending an encryption failure report. Changed the code to check for this particular request and send the wrong timeliness report instead.@@@Version 1.09@@@The descriptions in the interfaces MIB were switched. This was caused by the SNMP virtual table init function accessing the device list directly instead of by index. .Changed the way the device list is accessed in naSnmpinitVertualInterfaceTable(). Refactored the name of the loopback interface from LOOPBACK to lo. (NETOS-198)  Requires TCPIP fix v1.08@@@Instructions to recompile the MIB sample project after compiling the MIB were incomplete.  Changed readme files to be clearer.Fixed some typos in the readme files.  (NETOS-179)@@@tSNMP was starting with a timeslice of 0, starving other threads with the same priority and pre-emption threshold. Timeslice was changed to 1. (NETOS-197)@@@Version 1.10@@@tfInitializeEngine was being called twice, causing an overwrite to happen in memory address 0. This commit avoids this situation.  (NETOS-227)@@@Version 1.11@@@Required dependency of TCPIP Update version 1.11 for TRECK Security Fixes.   (NPIX-1141)
Minidescription: SNMP Updates since the release of NET+OS 7.5.2
platformversion: 7.5
Revision: 2
platform: netos
Relevance: CRITICAL
Filename: SNMP_Updates_752_130.dipk
Date: 12/05/2020
Type: fix
Target: environment
neededfiles: none
rootfs: none
Size: 13301kb
Installedsize: 29825kb
Checksum: 31a4728fc9ecdeff9a36c6c7361df74b
