ID: 24
Name: SNMP_Updates_742
Version: 1.95
Dependences: 20, 92
Description: Version 1.0@@@Calls to function naSnmpGetSysName() fail consistently with a return code of NA_SNMP_NO_MEMORY due to a typo in the source code. The function now returns NA_SUCCESS on success and NA_SNMP_NO_MEMORY on failure. (case 30083)@@@Added fflush() after fputs() to flush out the STDOUT writes in the SNMPv3 example apps CLI.@@@Version 1.1@@@Applied fixes to handle large sub ids while processing get requests, and for handling requests with bad lengths.@@@Applied changes for conceptual tables.@@@Version 1.2@@@Applied fixes to prevent failures while adding V3 Users. (case 30940)@@@Added namib3 example application.@@@Fixed write access in nasnmpv3 example application.@@@Version 1.3@@@Added fix from Treck to return the correct security level in a NotInTimeWindow SNMP report.@@@Version 1.4@@@Fixed viewing USM table and several other SNMPv3 tables. (case 31929)@@@Fixed adding users before SNMP agent has started. (case 31941)@@@Version 1.5@@@Fix for crash caused by the mismatch of TCPIP and SNMP libraries with and without IPSEC. (case 33312 )@@@Version 1.6@@@We get the following linker error, undefined reference to tfProcessUnsignedInt when unsigned ints are included in a MIB. Enabled TM_USE_PROCESS_UINT in SNMP agent to resolve issue. (case 33658)@@@If only one SNMPv3 user exists and it does not have an authentication protocol, that user will be denied access to the SNMP agent. Fixed access for user with no authentication protocol.  (case 33851)@@@Version 1.7@@@SMIDUMP.EXE@@@Fixed invalid indices generated by the MIB compiler. (case 34053)@@@MAKEINS.EXE@@@Fixed a problem with the instructions filename which could cause runtime errors with some MIBs. (case 34054)@@@Version 1.8@@@Added Error code for naSnmpDeleteTrap, when deleting 1st entry. (Case 35853)@@@Added snmpTargetMIB and snmpNotificationMIB API and callbacks.@@@This update is dependent on Common Updates Version 1.0@@@Version 1.9@@@Changed the nasnmpd example to use enterprise OID array of NaSnmpTrap_t structure. Changed autodoc for NaSnmpTrap_t structure. (Case 36249)@@@Version 1.91@@@Updated MIB-II extensions for IP, TCP and UDP to bring them in sync with Treck Agent.@@@Version 1.92@@@Updated MIB-II extensions for IP, INET-ADDRESS and UDP to bring them in sync with Treck Agent.@@@Updated the SNMP agent to use the short format for ASN1 item lengths when possible.  Previously the old code always encoded the length as 3 bytes.  Now it will be encoded as 1 byte if possible.@@@Version 1.93@@@Fix for snmp replying to a different IP address, than in received request (IPv6)  (Case 43127)@@@Version 1.94@@@Fixed MIB compiler hanging problem, when compiling ITU-MIB.mib (rfc 3877) (Case 44380) @@@Report correct Ethernet link speed in SNMP ifSpeed  (Case 41612)  Requires TCPIP fix v1.47.@@@Version 1.95@@@Replaced direct malloc() and free calls() with tm_snmp_malloc and tm_snmp_free in NET+OS snmpv3 api. (NETOS-39)
Minidescription: SNMP Updates for NET+OS 7.4.2
platformversion: 7.4
Revision: 2
platform: netos
Relevance: NORMAL
Filename: SNMP_Updates_742_24.dipk
Date: 14/04/2014
Type: fix
Target: environment
neededfiles: none
rootfs: none
Size: 14781kb
Installedsize: 35327kb
Checksum: 33e2abd19fb15451fb1e6d0050073dd3
